The Rtp-01a~01b, Rtp-02a~02b, Rtp-03a~ 03f & 04a~04f adapter's controller driver description as below:

     1. DOS       ---- for dos, it will be display and install board's address & irq under your computer environment.
                         (command form : NmDosIn /? )

     2. WINNT  ---- for board's driver under Windows Nt.
                        2.1 NetMosPCIDiagnostics : for board detect under Win Nt system.
                        2.2 Readme -- diagnostics program install guide. 
                        2.3 NetMosWinNtParPortDrivers : Win Nt driver program.

     3. WIN95   ---- for board's driver under Windows 95.

     4. WIN98   ---- for board's driver under Windows 98, see the file "Win 98 Driver Installation".

     5. WINME ---- for board's driver under Windows Me. 

     6. WINXP  ---- for board's driver under Windows Xp.
                        6.1 NetMosPCIDiagnostics : for board detect under Win Xp system.
                        6.2 Readme-1 : release note.
                        6.2 Readme-2 : diagnostics program install guide.

     7. WIN2000 ---- for board's driver under Windows 2000.
                          7.1 NetMosPCIDiagnostics : for board detect under Win Nt system.
                          7.2 Readme : diagnostics program install guide.  
   
      8. WIN2003 Server  ---- for board's driver under Windows 2003 Server.
                        8.1 NetMosPCIDiagnostics : for board detect under Win 2003Server system.
                        8.2 Readme-1 : release note.
                        8.2 Readme-2 : diagnostics program install guide.

      9. LINUX ---- for linux system install guide.

      10. All pci i/o card's driver can be supported to SLIM PC.

      11.The file " faq.html " is Frequently Asked Questions file, if your file is not complete, please download from:
                       http://www.moschip.com/faq.html

      12.All newer update driver, please contact with agent or download from :
                       http://www.moschip.com.drivers.html


        The driver download from chip's website:
       >> Rtp-03a pci dual serial card:  
        -- select 'products' -->  'PCI' --> 'Nm9835CV ____ Drivers,Release Notes and installation Guides'

       >> Rtp-03c pci dual rs422/485 card:
        -- select 'products' -->  'PCI' --> 'Nm9835CV ____ Drivers,Release Notes and installation Guides'

       >>  Rtp-04a pci multi serial card:     
        -- select 'products' -->  'PCI' --> 'Nm9845CV ____ Drivers,Release Notes and installation Guides'
 
       >>  Rtp-04c pci dual Rs485 & dual serial card:     
        -- select 'products' -->  'PCI' --> 'Nm9845CV ____ Drivers,Release Notes and installation Guides'
       



     Note:
     ========================================================================

    1. (Before driver and RTP-03x & RTP-04x  install --- mainboard BIOS (pnp os install)  DOS and Windows NT are the most operating system that PnP needs to be
     manual, other than that all others are auto PnP.

    2. Both of Win Nt & Linux driver download with force serial item.
